INSURANCE COMPANY REQUESTED REPAIRS/REPLACEMENT LIST PLEASE SEE REPAIRS DONE UNDER SAID REQUEST PICTURES ATTACHED IN EMAIL **
26-06 The hot lead for the shore power inlet is wired to an inlet breaker. The wiring inside the storage closet on the starboard side of the cockpit is exposed. This should be put in an electrical box or a protective cover so that nobody can make contact with the exposed wiring. SOLUTION: BOXED IN THE SHORE POWER WIRING SO IT CAN NOT BE TOUCHED OR CONTACTED **
26-09 All of the wood blocks for the vessel’s thru hull fittings and transducers have rotted wood that is badly deteriorated. It is recommended that all of the wood backing blocks be inspected. Any deteriorated or damaged backing blocks should be replaced. All of the thru hull fittings should be inspected as there is some evidence of corrosion. Any corroded thru hull fittings should be replaced SOLUTION: REPLACED/REPAIRED ALL NEEDED THRU HULLS AND WOOD BLOCKS THAT WERE ROTTING AND DETERIORATING **
26-10 There is some corrosion and weeping on the engine’s heat exchanger and some of the piping. The heat exchanger should be serviced, cleaned, re-gasketed and re-sealed. Any deteriorated hoses should be replaced. Any corroded piping should be cleaned and painted or replace SOLUTION: HOSES HAVE BEEN REPLACED AND HEAT EXCHANGER HAS BEEN ULTRASONICALLY CLEANED,PRESSURE TESTED AND RE-SEALED WITH NEW GASKETS **26-11 The engine’s exhaust hose shows early signs of deterioration SOLUTION: HOSE REPLACED W/NEW SHIELDSFLEX HOSE WITH CORRUGATED WIRE **
[bookmark: _GoBack]26-13 The vessel’s fuel system should be equipped with a bonding wire between the fuel tank and the metallic deck fill fitting to prevent the build up of static electricity when fueling. **26-25 The vessel’s bonding wires for the bonding system appear to be in the need of repair. The bonding wire should be checked and repaired SOLUTION: ALL BONDING HAS BEEN REPLACED WITH NEW WIRE,CRIMPS AND CONTACT AREAS WERE CLEANED & GREASED


NON FUNCTIONAL SEACOCKS AND CORRODED THROUGH HULL FITTINGS HAVE BEEN REPLACED WITH GROCO BRONZE TRI FLANGE SEACOCKS AND BRONZE THROUGH HULL FITTINGS ALL THRU HULL FITTINGS AND STARBOARD PADS HAVE BEEN BEDDED IN 3M 5200 HULL SURFACES WERE SANDED,PREPPED WITH ACETONE AND HOLES CHAMFERED ON THE EXTERIOR TO FORM A DONUT OF SEALANT AROUND THE THREADS OF THRU HULLS
[image: Attachment]  Strainer and thru hull  


[image: Attachment]Main engine, thru hull, seacock, strainer

SEE DETAIL OF PAD AND STUDS FOR SEACOCK AND BEDDING UNDER STARBOARD PAD DETAIL OF NEW BONDING WIRE AND CONNECTION
[image: Attachment]Waste valve with thru hull

[image: Attachment]Bilge pump manual override switches, with pump operation pilot lights




[image: Attachment]Bilge pumps, smaller deep keel and large high water pump.





[image: Attachment]Bilge pump manual and auto fuses, and bonding buss bar

[bookmark: _GoBack][image: Attachment]New bilge pump discharge thru hulls and bonding on fuel fill

[image: Attachment]Fuel tank bonding to buss and fuel fill fitting

[image: Attachment]Transom anode bolts, wiring, and seals... No leaks




INSURANCE COMPANY REQUESTED REPAIRS/REPLACEMENT LIST
PLEASE SEE REPAIRS DONE UNDER SAID REQUEST PICTURES ATTACHED IN EMAIL

**26-06 The hot lead for the shore power inlet is wired to an inlet breaker. The wiring inside the storage closet on the starboard side of the cockpit is exposed. This should be put in an electrical box or a protective cover so that nobody can make contact with the exposed wiring. 

SOLUTION: BOXED IN THE SHORE POWER WIRING SO IT CAN NOT BE TOUCHED OR CONTACTED

**26-09 All of the wood blocks for the vessel’s thru hull fittings and transducers have rotted wood that is badly deteriorated. It is recommended that all of the wood backing blocks be inspected. Any deteriorated or damaged backing blocks should be replaced. All of the thru hull fittings should be inspected as there is some evidence of corrosion. Any corroded thru hull fittings should be replaced 

SOLUTION: REPLACED/REPAIRED ALL NEEDED THRU HULLS AND WOOD BLOCKS THAT WERE ROTTING AND DETERIORATING 


**26-10 There is some corrosion and weeping on the engine’s heat exchanger and some of the piping. The heat exchanger should be serviced, cleaned, re-gasketed and re-sealed. Any deteriorated hoses should be replaced. Any corroded piping should be cleaned and painted or replace 

SOLUTION: HOSES HAVE BEEN REPLACED AND HEAT EXCHANGER HAS BEEN ULTRASONICALLY CLEANED,PRESSURE TESTED AND RE-SEALED WITH NEW GASKETS

**26-11 The engine’s exhaust hose shows early signs of deterioration 

SOLUTION: HOSE REPLACED W/NEW SHIELDSFLEX HOSE WITH CORRUGATED WIRE 

**26-13 The vessel’s fuel system should be equipped with a bonding wire between the fuel tank and the metallic deck fill fitting to prevent the build up of static electricity when fueling. 
**26-25 The vessel’s bonding wires for the bonding system appear to be in the need of repair. The bonding wire should be checked and repaired 

SOLUTION: ALL BONDING HAS BEEN REPLACED WITH NEW WIRE,CRIMPS AND CONTACT AREAS WERE CLEANED & GREASED WITH CORROSION PROTECTANT



Heat Exchanger with all new hose 
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